# Pneumatic Clutches

At Kathuria Techmech, we provide high-quality European-made pneumatic clutches specifically designed for hot steel rolling mills. Sourced from the world’s top manufacturers, these pneumatic clutches are built to deliver superior performance, durability, and precision under the intense demands of steel production environments.

These advanced clutches ensure smooth and reliable operation, minimizing downtime and maximizing productivity in your rolling mill processes. With a focus on efficiency and robust construction, these pneumatic clutches offer the perfect solution for maintaining optimal control and performance in hot steel rolling applications.

Torque: up to 25,000 Nm

Rotations per minute: 500 - 3,200 min-1

WOutside diameter: 166 - 1,285 mm

Bore diameter: 21 - 270 mm

Length: 48 - 662 mm

In steel rolling mills, these clutch-brake units are widely used in the operation of heavy-duty cold shears, which are essential for cutting finished materials to the desired lengths. Their reliability and precision make them ideal for handling the rigorous demands of steel processing, ensuring efficient and accurate cutting in high-performance environments.

## Contact Us

A-7/116, S.S.G.T. Road, Industrial Area
Ghaziabad - 201009 (U.P.), India.
kathuriatechmech@gmail.com, info@kathuriatechmech.com
+91 9711466783, +91 7719617471
in
LinkedIn Profile